| VELOSTER(FS) >2013 > G 1.6 GDI > Suspension System > Rear Suspension System > Rear Shock Absorber>Repair procedures |

Replacement
1. | Remove the rear wheel & tire.
Tightening torque : 88.3 ~ 107.9N.m (9.0 ~ 11.0kgf.m, 65.1 ~ 79.6lb-ft)
Be careful not to damage to the hub bolts when removing the rear wheel & tire.
2. | Remove the rear shock absorber (A) from the frame by loosening the bolt.
Tightening torque : 98.1 ~ 117.7N.m (10.0 ~ 12.0kgf.m, 72.3 ~ 86.8lb-ft)
3. | Loosen the bolt & nut and then remove the rear shock absorber (A) from the torsion beam axle (B).
Tightening torque : 98.1 ~ 117.7N.m (10.0 ~ 12.0kgf.m, 72.3 ~ 86.8lb-ft)
4. | Installation is the reverse of removal.
Inspection
1. | Check the components for damage or deformation.
2. | Compress and extend the piston and check that there is no abnormal resistance or unusual sound during operation.