| VELOSTER(FS) >2013 > G 1.6 GDI > Fuel System > Fuel Delivery System > Fuel Tank>Repair procedures |

Removal
1. | Release the residual pressure in fuel line (Refer to “Release Residual Pressure in Fuel Line” in this group).
2. | Remove the rear seat [LH] (Refer to “Seat” in BD group).
3. | Remove the fuel pump service cover (A).
4. | Disconnect the fuel pump connector (A).
5. | Disconnect the fuel feed tube quick connector (B).
6. | Disconnect the fuel tank pressure sensor connector (C).
7. | Disconnect the vapor tube (D).
8. | Lift the vehicle and support the fuel tank with a jack.
9. | Remove the center muffler assembly (Refer to “Intake And Exhaust System” in EM group).
10. | Disconnect the fuel filler hose (A).
11. | Remove the under cover (A) and the parking brake line installation bolt (B).
12. | Remove the fuel tank from the vehicle after removing the fuel tank band (A).
Installation
1. | Installation is reverse of removal.
Fuel tank band installation nut: 39.2 ~ 54.0 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)