| VELOSTER(FS) >2013 > G 1.6 GDI > Body Electrical System > Immobilizer System > Immobilizer Control Unit>Repair procedures |

Removal
1. | Disconnect the negative (-) battery terminal.
2. | Remove the crash pad lower panel. (Refer to the BD group - "Crash pad")
3. | Disconnect the connector of the immobilizer unit and then remove the immobilizer unit (A) after loosening the bolt. [USA] [CANADA]
Installation
1. | Install the immobilizer unit.
2. | Connector the immobilizer unit.
3. | Install the crash pad lower panel.