| VELOSTER(FS) >2013 > G 1.6 GDI > Heating,Ventilation, Air Conditioning > Blower > Blower Resistor>Repair procedures |

Inspection
1. | Measure terminal-to-terminal resistance of the blower resistor.
2. | measured resistance is not within specification, the blower resistor must be replaced. (After removing the resistor)
1. ML 2. MH | 3. LO 4. HI
Replacement
1. | Disconnect the negative (-) battery terminal.
2. | Disconnect the blower resistor connector and then remove the blower resistor (A) after loosening the mounting screws.
3. | Installation is the reverse order of removal.