| VELOSTER(FS) >2013 > G 1.6 T-GDI > Fuel System > Engine Control System > RCV Control Solenoid Valve>Repair procedures |

Inspection
1. | Turn the ignition switch OFF.
2. | Disconnect the RCV connector.
3. | Measure resistance between the RCV terminals 1 and 2.
4. | Check that the resistance is within the specification.
Specification: Refer to "Specification"
Removal
1. | Turn the ignition switch OFF and disconnect the battery negative (-) cable.
2. | Remove the air duck (A).
3. | Disconnect the cooling pan control connector (A) and cooling pan & RCV extension connector (B) from the bracket.
4. | Disconnect the RCV control solenoid valve connector (A) and vapor hoses (B).
5. | Remove the installation bolts (C) and then RCV control solenoid valve (D).
Installation
• | Install the component with the specified torques.
• | Note that internal damage may occur when the component is dropped. If the component has been dropped, inspect before installing.
1. | Installation is reverse of removal.
RCV control solenoid valve bracket installation bolt: 9.8 ~ 11.8 N.m (1.0 ~ 1.2 kgf.m, 7.2 ~ 8.7 lb-ft)