| VELOSTER(FS) >2013 > G 1.6 T-GDI > Body Electrical System > Seat Electrical > Power Seat Control Switch>Repair procedures |

Inspection
1. | With the lumbar support switch (A) in each position, make sure that continuity exists between the terminals below. If continuity is not as specified, replace the lumbar support switch.
Removal
1. | Disconnect the negative (-) battery terminal.
2. | Remove the seat side cover (A). (Refer to the BD group - "Front seat")
3. | Remove the power seat control switch connector.
4. | Remove the power seat control switch(A) after loosening the mounting screw.
Installation
1. | Connect the connector and install the power seat control switch.
2. | Install the seat cover.