| VELOSTER(FS) >2013 > G 1.6 T-GDI > Engine Mechanical System > Lubrication System > Oil Pump>Repair procedures |

Removal and Installation
1. | Remove the timing chain cover. (Refer to Timing System - "Timing Chain Cover")
2. | Remove the pump cover (A).
Tightening torque : 8.8 ~ 13.7N.m (0.9 ~ 1.4kgf.m, 6.5 ~ 10.1 lb-ft)
3. | Remove the inner rotor (B) and outer rotor (C).
4. | Install in the reverse order of removal.