| VELOSTER(FS) >2013 > G 1.6 T-GDI > Fuel System > Fuel Delivery System > Filler-Neck Assembly>Repair procedures |

Removal
1. | Remove the rear-LH wheel, tire, and the inner wheel house.
2. | Disconnect the fuel filler hose (A), the leveling hose (B) and the ventilation hose (C).
3. | Open the fuel filler door and unfasten the filler-neck assembly mounting screw (A).
4. | Remove the filler-neck assembly from the vehicle after removing the bracket mounting bolts (A).
Installation
1. | Installation is reverse of removal.
Filler-neck assembly installation bolt: 7.8 ~ 11.8 N.m (0.8 ~ 1.2 kgf.m, 5.8 ~ 8.7 lb-ft) Filler-neck assembly installation screw: 7.8 ~ 11.8 N.m (0.8 ~ 1.2 kgf.m, 5.8 ~ 8.7 lb-ft)