| VELOSTER(FS) >2013 > G 1.6 T-GDI > Suspension System > Tires/Wheels > Wheel>Repair procedures |

Hub Nut Tightening Sequence Tighten the hub nuts as follows.
Tightening torque : 88.3 ~ 107.9N.m (9.0 ~ 11.0kgf.m, 65.1 ~ 79.6lb-ft)
When using an impact gun, final tightening torque should be checked using a torque wrench.
Wheel Runout
1. | Jack up the vehicle and support it with jack stands.
2. | Measure the wheel runout with a dial indicator as illustated.
3. | Replace the wheel if the wheel runout exceeds the limit.
Type | Radius direction | Axis direction
Aluminium | 0.3mm (0.01in) | 0.3mm (0.01in)