| VELOSTER(FS) >2013 > G 1.6 T-GDI > Fuel System > Engine Control System > RCV Control Solenoid Valve>Description and Operation |

Description
RCV (Recirculation Valve) Control Solenoid Valve is installed on the cooling pan motor top and operates the RCV actuator which controls the by-pass passage of the turbo-charger compressor. When the throttle valve is closed during engine running [Tip-out], crash noise of the impeller will occur because of rapid increasing of the boost pressure. So, in this case, in order to prevent this phenomenon, ECM maintains the appropriate boost pressure by opening the by-pass passage.