| VELOSTER(FS) >2013 > G 1.6 T-GDI > Body Electrical System > Panoramaroof > Panoramaroof Switch>Repair procedures |

Inspection
1. | Disconnect the negative (-) battery terminal.
2. | Open the sunglass case cover from the overhead console then remove the 2 screws holding the overhead console. Disconnect the switch connector (6P) and then remove the overhead console lamp.
3. | Check for continuity between the terminals. If the continuity is not as specified, replace the sunroof switch