| VELOSTER(FS) >2013 > G 1.6 T-GDI > Engine Electrical System > Ignition System > Ignition Coil>Repair procedures |

Removal
1. | Disconnect the battery nagative terminal.
2. | Remove the engine cover.
3. | Disconnect the ignition coil connector (A).
• | When removing the ignition coil connector, pull the lock pin (A) and push the clip (B).
4. | Remove the ignition coil (A).
Installation
1. | Install in the reverse order of removal.
Ignition coil installation bolts: 9.8 ~ 11.8 N.m (1.0 ~ 1.2 kgf.m, 7.2 ~ 8.7 Ib-ft)
Inspection
1. | Measure the primary coil resistance between terminals (+) and (-).
Standard value: 0.79Ω ± 15%