| VELOSTER(FS) >2013 > G 1.6 T-GDI > Body Electrical System > Back view camera System>Description and Operation |

Description
Back view camera will activate when the backup light is ON with the ignition switch ON and the shift lever in the R position. This system is a supplemental system that shows behind the vehicle through the AV monitor while backing-up.
This system is a supplementary function only. It is the responsibility of the driver to always check the inside/ outside rearview mirror and the area behind the vehicle before and during backing up because there are blind spots that can't be seen through the camera.