| VELOSTER(FS) >2013 > G 1.6 T-GDI > Fuel System > Engine Control System > Ambient Temperature Sensor (ATS)>Repair procedures |

Inspection
1. | Turn the ignition switch OFF.
2. | Disconnect the ATS connector.
3. | Measure resistance between the ATS terminals 1 and 2 [B1/S1].
4. | Check that the resistance is within the specification.
Specification: Refer to "Specification"
Removal
1. | Turn the ignition switch OFF and disconnect the battery negative (-) cable.
2. | Disconnect the Ambient Temperature Sensor connect (A).
3. | Remove the Ambient Temperature Sensor bracket (B).
Installation
• | Note that internal damage may occur when the component is dropped. If the component has been dropped, inspect before installing.
1. | Installation is reverse of removal.