| VELOSTER(FS) >2013 > G 1.6 T-GDI > Body Electrical System > Power Windows > Power Window Switch>Repair procedures |

Inspection
Power Window Main Switch Inspection
1. | Disconnect the negative (-) battery terminal.
2. | Remove the front door trim panel. (Refer to the BD group - "Front door")
3. | Check for continuity between the terminals in each switch position according to the table. If the continuity condition is not normal, replace the switch. [Auto Down] [Safety Up/Down]
4. | Remove the grip holder cover after loosening 4 bolts.
5. | Remove the grip holder bracket (A).
6. | Remove the power window switch module (A) after loosening 4 screws.
Passenger Power Window Switch Inspection
1. | Disconnect the negative (-) battery terminal.
2. | Remove the front door trim panel. (Refer to the BD group - "Front door")
3. | Disconnect the connector from the switch.
4. | Check for continuity between the terminals in each switch position according to the table. If the continuity condition is not normal, replace the switch.
5. | Remove the power window switch after loosening 2 screws.
Rear Power Window Switch Inspection
1. | Disconnect the negative (-) battery terminal.
2. | Remove the rear door trim panel. (Refer to the BD group - "Rear door")
3. | Disconnect the connector from the switch.
4. | Check for continuity between the terminals in each switch position according to the table. If the continuity condition is not normal, replace the switch.
5. | Remove the power window switch after loosening 2 screws.