| VELOSTER(FS) >2013 > G 1.6 T-GDI > Engine Mechanical System > Cooling System > Water Pipe>Repair procedures |

Removal and Installation
1. | Remove the water temperature control assembly. (Refer to Colling System - "Water Temperature Control Assembly")
2. | Remove the water pipe(A).
Tightening torque M6 bolt and nuts : 9.8 ~ 11.8N.m (1.0 ~ 1.2kgf.m, 7.2 ~ 8.7lb-ft) M8 bolt : 18.6 ~ 23.5N.m (1.9 ~ 2.4kgf.m, 13.7 ~ 17.4lb-ft)
3. | Install in the reverse order of removal.