| VELOSTER(FS) >2013 > G 1.6 T-GDI > Fuel System > Fuel Delivery System > Fuel Filter>Repair procedures |

Replacement
1. | Remove the fuel pump. (Refer to Fuel Delivery System - "Fuel Pump")
2. | Disconnect the electric motor pump connector (A) and the fuel sender connector (B).
3. | Remove the head assembly (D) after remove the fixing clip (C) of the cushion pipe.
4. | Remove the return nozzle (B) after releasing the hook (A).
5. | Remove the reserver-cup (B) after releasing the hook (A).
6. | Remove the pre-filter (C) after releasing the hook (A, B).
7. | Remove the electric motor pump (A) from the fuel filter (B) by pulling it in down direction.
8. | Replace new fuel filter.