| VELOSTER(FS) >2013 > G 1.6 T-GDI > Engine Mechanical System > Timing System > Timing Chain>Repair procedures |

Removal
1. | Turn the crankshaft pulley clockwise, and align its groove with the timing mark of the timing chain cover.
2. | Remove the timing chain cover. (Refer to Timing System - "Timing Chain Cover")
3. | Align the timing marks of the CVVT sprockets with the upper surface of the cylinder head to make No.1 cylinder be positioned at TDC.
Check the dowel pin of the crankshaft for facing upside of the engine at this monent.
4. | Remove the timing chain (A).
Before removing the tensioner, fix the piston of the tensioner with a pin through the hole(B) at compressed position.
5. | Remove the timing chain tensioner arm (A) and guide (B).
6. | Remove the timing chain (A).
Inspection
Sprockets, Hydraulic Tensioner, Chain Guide, Tensioner Arm, Timing Chain
1. | Check the CVVT sprocket, crankshaft sprocket teeth for abnormal wear, cracks or damage. Replace if necessary.
2. | Check a contact surface of the chain tensioner arm and guide for abnormal wear, cracks or damage. Replace if necessary.
3. | Check the hydraulic tensioner for its piston stroke and ratchet operation. Replace if necessary.
4. | Check the timing chain for its elongation, abnormal wear or damage. Replace if necessary.
Installation
1. | Dowel pin of crankshaft should be positioned at 3° in relation to vertical center line.
2. | Align the TDC marks (A) of the CVVT sprockets with the upper surface of the cylinder head to make No.1 cylinder be positioned at TDC.
3. | Install the new O-rings (A).
4. | Install the timing chain guide (A) and the timing chain (B).
Tightening torque : 9.8 ~ 11.8 N.m (1.0 ~ 1.2 kgf.m, 7.2 ~ 8.7 lb-ft)
• | When installing a timing chain, align the timing marks on the sprockets with paint marks of the chain.
• | Order : Crankshaft sprocket → Timing chain guide → Intake CVVT sprocket → Exhaust CVVT sprocket.
5. | Install the chain tensioner arm (A).
Tightening torque : 9.8 ~ 11.8 N.m (1.0 ~ 1.2 kgf.m, 7.2 ~ 8.7 lb-ft)
6. | Install the hydraulic tensioner (A) and remove the pin (B).
Tightening torque : 9.8 ~ 11.8 N.m (1.0 ~ 1.2 kgf.m, 7.2 ~ 8.7 lb-ft)
Recheck the top dead center (TDC) marks on the crankshaft and camshaft.
7. | Install the timing chain cover.