| VELOSTER(FS) >2013 > G 1.6 T-GDI > Restraint (Depowered) > Seat Belt Pretensioner > Seat Belt Pretensioner (BPT)>Repair procedures |

Removal
1. | Disconnect the battery negative cable, and wait for at least three minutes before beginning work.
2. | Remove the lower anchor bolt.
3. | Remove the following parts. (Refer to the Body group - "Interior trim")
A. | Door scuff trim
B. | Center pillar trim
4. | Remove the upper anchor bolt.
5. | Disconnect the seat belt pretensioner connector (A).
6. | Loosen the seat belt pretensioner mounting bolts (B,C) and remove the seat belt pretensioner.
Installation
1. | Remove the ignition key from the vehicle.
2. | Disconnect the battery negative cable and wait for at least three minutes.
3. | Install the seat belt pretensioner with a bolts (B, C).
Tightening torque [Bolt B]: 39.2 ~ 54.0 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)
4. | Connect the seat belt pretensioner (BPT) connector (A).
5. | Install the upper anchor bolts.
Tightening torque: 39.2 ~ 54.0 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)
6. | Install the following parts. (Refer to the Body group - "Interior trim")
A. | Center pillar trim
B. | Door scuff trim
7. | Install the lower anchor bolts.
Tightening torque: 39.2 ~ 54.0 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)
8. | Reconnect the battery negative cable.
9. | After installing the seat belt pretensioner, confirm proper system operation:
A. | Turn the ignition switch ON; the SRS indicator light should be turned on for about six seconds and then go off.