| VELOSTER(FS) >2013 > G 1.6 T-GDI > Body Electrical System > AVN System > GPS Antenna>Repair procedures |

Removal
Roof Antenna (GPS)
1. | Remove the rear roof trim. (Refer to the BD group - "Roof trim")
2. | Disconnect the cables (A) from the roof antenna.
3. | Remove the roof antenna (A) after removing a nut.
Installation
Roof Antenna (GPS)
1. | Install the roof antenna.
2. | Connect the GPS cable.
3. | Install the nut.
4. | Install the rear roof trim.
- | Make sure that the cables and connectors are plugged in properly.
- | Check the AVN system.