| VELOSTER(FS) >2013 > G 1.6 T-GDI > Fuel System > Engine Control System > Manifold Absolute Pressure Sensor (MAPS)>Repair procedures |

Inspection
1. | Connect the GDS on the Data Link Connector (DLC).
2. | Measure the output voltage of the MAPS at idle and IG ON.
Specification: Refer to "Specification"
Removal
1. | Turn the ignition switch OFF and disconnect the battery negative (-) cable.
2. | Disconnect the manifold absolute pressure sensor connector (A).
3. | Remove the installation bolt (B), and then remove the sensor from the surge tank.
Installation
• | Install the component with the specified torques.
• | Note that internal damage may occur when the component is dropped. If the component has been dropped, inspect before installing.
• | Insert the sensor in the installation hole and be careful not to damage.
1. | Installation is reverse of removal.
Manifold absolute pressure sensor installation bolt: 9.8 ~ 11.8 N.m (1.0 ~ 1.2 kgf.m, 7.2 ~ 8.7 lb-ft)