| VELOSTER(FS) >2013 > G 1.6 T-GDI > Engine Mechanical System > Lubrication System > Oil Pressure Switch>Repair procedures |

Removal and Installation
1. | Remove the under cover.
2. | Remove the oil drain plug, and drain the oil into a container.
3. | Remove the oil pressure switch(A).
Tightening torque : 7.8 ~ 11.7 N.m (0.8 ~ 1.2 kgf.m, 5.7 ~ 8.6 lb-ft)
4. | Install in the reverse order of removal.
Inspection
1. | Check the continuity between the terminal and the body with an ohmmeter. If there is no continuity, replace the oil pressure switch.
2. | Check the continuity between the terminal and the body when the fine wire is pushed. If there is continuity even when the fine wire is pushed, replace the switch.
3. | If there is no continuity when a 49.0kpa (0.5kg/cm², 7.1psi) is applied through the oil hole, the switch is operating properly. Check for air leakage. If air leaks, the diaphragm is broken. Replace it.