| VELOSTER(FS) >2013 > G 1.6 T-GDI > Engine Electrical System > Charging System > Battery>Description and Operation |

Description
1. | The MF(Maintenance Free) battery is, as the name implies, totally maintenance free and has no removable battery cell caps.
2. | The MF(Maintenance Free) battery does not require water replenishment for the repair.
3. | The battery is completely sealed, except for small vent holes in the cover.
• | After disconnecting then reconnecting the battery negative cable, reset some parts that require the reset procedures. (Refer to Body Electrical System – "General Information")