| VELOSTER(FS) >2013 > G 1.6 T-GDI > Body Electrical System > Rear Glass Defogger > Rear Glass Defogger Switch>Repair procedures |

Inspection
1. | The rear glass defogger switch inputs can be checked using the GDS.
2. | To check the input value of rear glass defogger switch, select option "Body Control Module".
3. | To consult the present input/output value of BCM, "Current DATA". It provides information of BCM input/output conditions of smart junction box.
4. | To check the input value of rear glass defogger switch in force mode, select option "Actuation Test of smart junction box".
Removal
1. | Disconnect the negative(-) battery terminal.
2. | Remove the center fascia panel assembly (A). (Refer to the Body group - "Crash pad")
3. | Remove the center fascia panel connector (A).
4. | Remove the heater and air corditioner controller (A), after loosening the screw (4EA).
Installation
1. | Install the heater and air conditioner controller to the center fascia panel.
2. | Install the center fascia panel assembly.