| VELOSTER(FS) >2013 > G 1.6 T-GDI > Body (Interior and Exterior) > Exterior > Fender>Repair procedures |

Replacement
• | When removing and installing the fender, an assistant is necessary.
• | Be careful not to damage the fender and body.
• | When removing the clips, use a clip remover.
1. | Remove the front bumper cover. (Refer to the BD group – “Front bumper”)
2. | Remove the head lamps. (Refer to the BE group – “Head Lamps”)
3. | Loosen the mud guard (A) mounting screws and clips.
4. | To remove the A pillar garnish (A), loosen the mounting screw after removing the cap (B).
Tightening torque : 0.5 ~ 1.0N.m (0.05 ~ 0.1kgf.m, 0.4 ~ 0.7 lb-ft)
5. | Detach the clip and then remove the fender side cover (A).
6. | Detach the clips and then remove the insulator pad (A).
7. | After loosening the mounting screws and bolt, then remove the front bumper side mounting bracket (A).
8. | After loosening the mounting bolts and nut, then remove the fender (A).
9. | Installation is the reverse of removal.