| VELOSTER(FS) >2013 > G 1.6 T-GDI > Engine Mechanical System > Cooling System > Radiator Hose>Repair procedures |

Removal and Installation
1. | Loosen the drain plug, and drain the engine coolant. Remove the radiator cap to drain with speed.
2. | Disconnect the radiator upper hose (A) and lower hose (B).
Install the radiator hoses as shown illustrations.
3. | Install in the reverse order of removal.