| VELOSTER(FS) >2013 > G 1.6 T-GDI > Body Electrical System > Lighting System > Overhead Console Lamp>Repair procedures |

Inspection
1. | Remove the overhead console lamp (map lamp) assembly then check for continuity between terminals. If the continuity is not as specified, replace the map lamp switch. [Overhead console] [Map lamp]
Removal
1. | Disconnect the negative (-) battery terminal.
2. | Loosen 2 screws holding the overhead console (A). Remove the overhead console (A) after loosening 2 screws.
3. | Disconnect the connectors (A) of sunroof switch and lamp switch then remove the overhead console lamp assembly.
4. | If necessary to replace the bulb, replace the bulb after removing the overhead console lens (A).
Installation
1. | Install the overhead console lamp.
2. | Connect the sunroof switch connector and lamp connector.
3. | Install the overhead console assembly.