| VELOSTER(FS) >2013 > G 1.6 T-GDI > Engine Mechanical System > Timing System > Drive Belt Tensioner>Repair procedures |

Removal and Installation
1. | Remove the drive belt. (Refer to Timing System - "Dreve Belt")
2. | Remove the alternator. (Refer to Engine Electrical System - "Alternator")
3. | Remove the alternator bracket(belt tunsioner)(A).
Tightening torque : 19.6 ~ 26.5 N.m (2.0 ~ 2.7 kgf.m, 14.5 ~ 19.5 lb-ft)
4. | Install in the reverse order of removal.