| VELOSTER(FS) >2013 > G 1.6 T-GDI > Body Electrical System > AVN System > Multimedia Jack>Repair procedures |

Removal
1. | Remove the floor console assembly. (Refer to the BD group - "Console")
2. | Remove the multimedia jack assembly (A).
3. | Disconnect the multimidia jack connector (A).
4. | Remove the multimedia jack (B)after releasing the fixed hooks (A).
Installation
1. | Install the multimedia jack.
2. | Install the floor console assembly.
Make sure the multimedia connector and the console upper cover connectors are plugged in properly.