| VELOSTER(FS) >2013 > G 1.6 T-GDI > Engine Mechanical System > Cooling System > Heater Hose>Repair procedures |

Removal and Installation
1. | Loosen the drain plug, and drain the engine coolant. Remove the radiator cap to drain with speed.
2. | Disconnect the mounting clamp and then remove the heater hose(A).
3. | Remove the heater hoses (A).
Install the heater hoses as shown illustrations.
4. | Install in the reverse order of removal.