| VELOSTER(FS) >2013 > G 1.6 T-GDI > Body (Interior and Exterior) > General Information>Specifications |

Specifications
Items | Specification
Hood | Type | Rear hinged, front opening type
Front Door | Construction | Front hinged, full door construction
Regulator system | Wire-drum type
Locking system | Pin-fork system
Rear Door | Construction | Front hinged, full door construction
Regulator system | Wire-drum type
Locking system | Pin-fork system
Tail Gate | Type | Front hinged, gas lifter type
Seat Belts | Front | 3 point type with Emergency Locking Retractor (E.L.R)
Rear | 3 point type with Emergency Locking Retractor (E.L.R) 2 point type
Tightening Torque
Items | N.m | kgf.m | lb-ft
Front and rear doors | Door hinge to body | 34.3 ~ 41.2 | 3.5 ~ 4.2 | 25.3 ~ 30.4
Door hinge to door | 21.6 ~ 26.5 | 2.2 ~ 2.7 | 15.9 ~ 19.5
Door checker to door | 6.9 ~ 10.8 | 0.7 ~ 1.1 | 5.1 ~ 8.0
Door checker to body | 16.7 ~ 21.6 | 1.7 ~ 2.2 | 12.3 ~ 15.9
Door trim mounting bolts | 7.8 ~ 11.8 | 0.8 ~ 1.2 | 5.8 ~8.7
Door glass mounting bolt | 7.8 ~ 11.8 | 0.8 ~ 1.2 | 5.8 ~ 8.7
Outside handle base mounting bolt | 7.8 ~ 10.8 | 0.8 ~ 1.1 | 5.8 ~ 8.0
Door outside handle mounting bolts | 7.8 ~ 11.8 | 0.8 ~ 1.2 | 5.8 ~8.7
Door channel mounting nuts | 3.9 ~ 5.9 | 0.4 ~ 0.6 | 2.9 ~ 4.3
Latch mounting bolts | 7.8 ~ 10.8 | 0.8 ~ 1.1 | 5.8 ~ 8.0
Door regulator mounting bolts | 3.9 ~ 5.9 | 0.4 ~ 0.6 | 2.9 ~ 4.3
Door striker mounting bolts | 16.7 ~ 21.6 | 1.7 ~ 2.2 | 12.3 ~ 15.9
Tail gate | Tail gate hinge to tail gate | 21.6 ~ 26.5 | 2.2 ~ 2.7 | 15.9 ~ 19.5
Tail gate hinge to body | 21.6 ~ 26.5 | 2.2 ~ 2.7 | 15.9 ~ 19.5
Tail gate latch mounting bolts | 6.9 ~ 10.8 | 0.7 ~ 1.1 | 5.1 ~ 8.0
Tail gate striker mounting bolts | 21.6 ~ 26.5 | 2.2 ~ 2.7 | 15.9 ~ 19.5
Hood | Hood hinge to body | 21.6 ~ 26.5 | 2.2 ~ 2.7 | 15.9 ~ 19.5
Hood hinge to hood | 21.6 ~ 26.5 | 2.2 ~ 2.7 | 15.9 ~ 19.5
Hood latch to body mounting bolts | 7.8 ~ 11.8 | 0.8 ~ 1.2 | 5.8 ~8.7
Seat | Front seat mounting bolts | 34.3 ~ 53.9 | 3.5 ~ 5.5 | 25.3~ 39.8
Front seat frame mounting bolts | 49.0 ~ 63.7 | 5.0 ~ 6.5 | 36.2~ 47.0
Rear seat mounting bolts | 16.7 ~ 25.5 | 1.7 ~ 2.6 | 12.3 ~ 18.8
Rear seat latch mounting bolts | 19.6 ~ 29.4 | 2.0 ~ 3.0 | 14.5 ~ 21.7
Seat belt | Height adjuster mounting bolts | 39.2 ~ 53.9 | 4.0 ~ 5.5 | 28.9 ~ 39.8
Front seat belt upper anchor mounting bolt | 39.2 ~ 53.9 | 4.0 ~ 5.5 | 28.9 ~ 39.8
Anchor pretensioner mounting bolt | 39.2 ~ 53.9 | 4.0 ~ 5.5 | 28.9 ~ 39.8
Front seat belt retractor mounting bolt | 39.2 ~ 53.9 | 4.0 ~ 5.5 | 28.9 ~ 39.8
Rear seat belt lower anchor mounting bolt | 39.2 ~ 53.9 | 4.0 ~ 5.5 | 28.9 ~ 39.8
Rear seat belt retractor mounting bolt | 39.2 ~ 53.9 | 4.0 ~ 5.5 | 28.9 ~ 39.8
Seat belt buckle mounting bolt | 39.2 ~ 53.9 | 4.0 ~ 5.5 | 28.9 ~ 39.8
Outside rearview mirror | Outside rearview mirror mounting bolts | 3.9 ~ 5.9 | 0.4 ~ 0.6 | 2.9 ~ 4.3
Wiper arm | Wiper arm mounting nuts | 22.6 ~ 26.5 | 2.3 ~ 2.7 | 16.6 ~ 19.5
Hood garnish | Hood garnish mounting nuts | 3.9 ~ 4.4 | 0.4 ~ 0.45 | 2.9 ~ 3.3
A Pillar garnish | A Pillar garnish mounting screw | 0.5 ~ 1.0 | 0.05 ~ 0.1 | 0.4 ~ 0.7
Rear spoiler | Rear spoiler mounting nuts | 5.9 ~ 6.4 | 0.6 ~ 0.65 | 4.3 ~ 4.7
Quarter fixed glass | Quarter fixed glass mounting nuts | 3.9 ~ 4.4 | 0.4 ~ 0.45 | 2.9 ~ 3.3
Panoramaroof | Panoramaroof mounting nuts | 6.9 ~ 10.8 | 0.7 ~ 1.1 | 5.1 ~ 8.0
Panoramaroof mounting bolts | 10.8 ~ 13.7 | 1.1 ~ 1.4 | 8.0 ~ 10.1