| VELOSTER(FS) >2013 > G 1.6 T-GDI > Engine Mechanical System > Engine And Transmission Assembly > Engine Mounting>Repair procedures |

Removal and Installation
Rollroad Mounting
1. | Rollroad bracket mounting bolts and rollroad bracket(A).
Tightening torque Nut (B) : 107.9 ~ 127.5 N.m (11.0 ~ 13.0 kgf.m, 79.6 ~ 94.0 lb-ft) Bolt (C) : 49.0 ~ 63.7 N.m (5.0 ~ 6.5 kgf.m, 36.2 ~ 47.0 lb-ft)
2. | Remove the rollroad supprt bracket(D).
Tightening torque: 49.0 ~ 68.6 N.m (5.0 ~ 7.0 kgf.m, 36.2 ~ 50.6 lb-ft)
3. | Install in the reverse order of removal.
Engine Mounting Support Bracket
1. | Disconnect the ground cable.
Tightening torque Ground line bolt : 10.8 ~ 13.7 N.m (1.1 ~ 1.4 kgf.m, 8.0 ~ 10.1 lb-ft)
2. | Install the jack to the edge of upper oil pan to support the engine.
Insert the rubber block between jack and oil pan.
3. | Remove the engine mounting support bracket (A).
Tightening torque Nut (B) : 63.7 ~ 83.4 N.m (6.5 ~ 8.5 kgf.m, 47.0 ~ 61.5 lb-ft) Bolt and nuts (C) : 49.0 ~ 63.7 N.m (5.0 ~ 6.5 kgf.m, 36.2 ~ 47.0 lb-ft)
4. | Install in the reverse order of removal.