| VELOSTER(FS) >2013 > G 1.6 T-GDI > Body (Interior and Exterior) > Interior > Roof Trim>Repair procedures |

Replacement
Sunvisor Replacement
• | Use a plastic panel removal tool to remove interior trim pieces to without marring the surface.
• | Put on gloves to protect your hands.
1. | After loosening the mounting screws, then remove the sunvisor (A) and retainer (B).
2. | Installation is the reverse of removal.
Assist Handle Replacement
• | Use a plastic panel removal tool to remove interior trim pieces to without marring the surface.
• | Put on gloves to protect your hands.
1. | Remove the covers (A).
2. | After loosening the mounting screws, then remove the assist handle (B).
3. | Installation is the reverse of removal.
Garment Hook Assembly Replacement
• | Use a plastic panel removal tool to remove interior trim pieces to without marring the surface.
• | Put on gloves to protect your hands.
1. | Remove the cover (B).
2. | After loosening the mounting bolt, then remove the garment hook assembly (A).
3. | Installation is the reverse of removal.
Overhead Console Replacement
• | Use a plastic panel removal tool to remove interior trim pieces to without marring the surface.
• | Put on gloves to protect your hands.
1. | After loosening the mounting screws, then remove the overhead console assembly (A).
2. | Disconnect the connectors (A).
3. | Installation is the reverse of removal.
• | Make sure the connector is connected properly.
Vanity Lamp Replacement
• | Use a plastic panel removal tool to remove interior trim pieces to protect from marring the surface.
• | Put on gloves to protect your hands.
1. | Using a screwdriver or remover, remove the vanity lamp (A).
2. | Disconnect the vanity lamp connector (B).
3. | Installation is the reverse of removal.
• | Make sure the connector is plugged in properly.
• | Replace any damage clips.
Roof Trim Replacement
• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Put on gloves to protect your hands.
1. | Remove the following items.
A. | Front seat (Refer to the BD group - "Front Seat")
B. | Rear seat (Refer to the BD group - "Rear Seat")
C. | Sunvisor
D. | Overhead console
E. | Garment hook assembly
F. | Assist handle
G. | Front pillar trim (Refer to the BD group - " Interior Trim")
H. | Front door scuff trim & Rear door scuff trim (Refer to the BD group - " Interior Trim")
I. | Center pillar lower trim & Center pillar upper trim (Refer to the BD group - " Interior Trim")
J. | Luggage side trim (Refer to the BD group - " Interior Trim")
K. | Rear pillar trim (Refer to the BD group - " Interior Trim")
2. | Remove the ECM mirror cover (B).
3. | Disconnect the ECM mirror connector (A).
4. | Disconnect the connector (A) and the mounting clips in the front pillar.
5. | Remove the clips and roof trim (A).
6. | Installation is the reverse of removal.
• | Make sure the connectors are plugged in properly.
• | Replace any damage clips.