| VELOSTER(FS) >2013 > G 1.6 T-GDI > Body Electrical System > AVN System>Specifications |

Specifications
Item | Specification
Power source | DC 14.4V (-) ground
Frequency range | FM : 87.5 ~ 107.9 MHz / 200 kHz AM : 530 ~ 1710 kHz / 10 kHz
Tuning type | PLL SYNTHESIZED TUNING
Antenna | 80 pF 75 Ohm
Dark current | MAX 4mA (Head unit only)
S/N | FM : MIN 50 dB AM : MIN 40 dB
Display System
Input signal | Digital RGB
Size | 7 inch