| VELOSTER(FS) >2013 > G 1.6 T-GDI > Engine Mechanical System > Cooling System > Cooling Fan>Repair procedures |

Removal and Installation
1. | Disconnect the battery negative terminal.
2. | Remove the air cleaner assembly. (Refer to Intake and exhaust system - "Air Cleaner")
3. | Disconnect the over flow hose (A) from the radiator.
4. | Disconnect the ATF cooler hose from cooling fan.
5. | Remove the front bumper. (Refer to Body - "Front Bumper")
6. | Remove the head lamp. (Refer to Body Electrical System - "Head Lamp")
7. | Remove the radiator upper bracket (A).
8. | Disconnect the cooling fan controller connector (A).
9. | Remove the filler neck assembly bolts(A).
10. | Remove the cooling fan assembly (B) from radiator (A).
Tightening torque : 4.9 ~ 7.8 N.m (0.5 ~ 0.8 kgf.m, 3.6 ~ 5.7 lb-ft)
11. | Install in the reverse order of removal.