| VELOSTER(FS) >2013 > G 1.6 T-GDI > Fuel System > Engine Control System > Heated Oxygen Sensor (HO2S)>Specifications |

Specification
HO2S [Bank 1/Sensor 1] (Linear type)
Item | Specification
Heater Resistance (Ω) | 2.4 ~ 4.0 [20°C(68°F)]
Item | Specification
Heater Resistance (Ω) | Approx. 9.0 [20°C(68°F)]
HO2S [Bank 1/Sensor 2] (Binary type)
A/F Ratio (λ) | Output Voltage(V)
RICH | 0.6 ~ 1.0
LEAN | 0 ~ 0.4
Item | Specification
Heater Resistance (Ω) | Approx. 9.0 [20°C(68°F)]