| VELOSTER(FS) >2013 > G 1.6 T-GDI > Body Electrical System > Power Door Mirrors > Power Outside Mirror Switch>Repair procedures |

Inspection
1. | Disconnect the power door mirror switch module connector from front door trim panel.
2. | Check for the continuity between terminals of power door mirror switch according to the table. [Power Mirror Switch]
Removal
1. | Disconnect the negative(-) battery terminal.
2. | Remove the front door trim panel. (Refer to the BD group - "Front door")
3. | Disconnect the power door mirror switch connector(A) from the door trim panel.
4. | Remove the power door mirror switch(A), after loosening the screw (3EA).
Be careful not to damage the hook when removing the switch module.
Installation
1. | Install the driver power window switch and connectors.
2. | Install the front door trim panel.