| VELOSTER(FS) >2013 > G 1.6 T-GDI > Emission Control System > Evaporative Emission Control System > Fuel Tank Air Filter>Repair procedures |

Removal
1. | Turn the ignition switch OFF and disconnect the battery negative (-) cable.
2. | Lift the vehicle.
3. | Disconnect the canister close valve connector (A).
4. | Disconnect the ventilation hose (B) from the fuel tank air filter and canister close valve.
5. | Remove the fuel tank air filter assembly after removing bolts (C).
6. | Release the lever (A), and then separate the canister close valve (B) from the fuel tank air filter (C) after rotating it in the direction of the arrow in the figure.
Installation
• | Install the component with the specified torques.
• | Note that internal damage may occur when the component is dropped. In this case, use it after inspecting.
1. | Installation is reverse of removal.