| VELOSTER(FS) >2013 > G 1.6 T-GDI > Fuel System > Engine Control System > Crankshaft Position Sensor (CKPS)>Repair procedures |

Inspection
1. | Check signal waveform of CKPS and CMPS using a GDS.
Specification: Refer to “Waveform”
Removal
1. | Turn the ignition switch OFF and disconnect the battery negative (-) cable.
2. | Disconnect the crankshaft position sensor connector (A) and remove the sensor (B) after removing the installation bolt.
Installation
• | Install the component with the specified torques.
• | Note that internal damage may occur when the component is dropped. If the component has been dropped, inspect before installing.
• | Apply the engine oil to the O-ring.
• | Insert the sensor in the installation hole and be careful not to damage.
1. | Installation is reverse of removal.
Crankshaft position sensor installation bolt: 7.8 ~ 11.8 N.m (0.8 ~ 1.2 kgf.m, 5.8 ~ 8.7 lb-ft)