| VELOSTER(FS) >2013 > G 1.6 T-GDI > Heating,Ventilation, Air Conditioning > Blower > Blower Unit>Repair procedures |

Replacement
1. | Disconnect the negative (-) battery terminal.
2. | Remove the heater & blower unit. (Refer to HA group - "Heater Unit")
3. | Remove the blower unit (A) from the heater unit after loosening a mounting screws.
Make sure that there is no air leaking out of the blower and duct joints
4. | Installation is the reverse order of removal.