| VELOSTER(FS) >2013 > G 1.6 T-GDI > Fuel System > Fuel Delivery System > Accelerator Pedal>Repair procedures |

Removal
1. | Turn the ignition switch OFF and disconnect the negative (-) battery cable.
2. | Disconnect the accelerator position sensor connector (A).
3. | Remove the installation bolt (B), the nuts (C) and then remove the accelerator pedal module.
Installation
1. | Installation is reverse of removal.
Accelerator pedal module installation nut: 9.8 ~ 14.7 N.m (1.0 ~ 1.5 kgf.m, 7.2 ~ 10.8 lb-ft) Accelerator pedal module installation bolt: 8.8 ~ 13.7 N.m (0.9 ~ 1.4 kgf.m, 6.5 ~ 10.1 lb-ft)