| VELOSTER(FS) >2013 > G 1.6 T-GDI > Brake System > ESC(Electronic Stability Control) System > ESC OFF Switch>Repair procedures |

Inspection
1. | Turn ignition switch OFF and disconnect the negative (-) battery cable.
2. | Remove the crash pad lower panel. (Refer to the Body group - "Crash pad")
3. | Remove the crash pad side switch assembly (A).
4. | Check the continuity between the switch terminals as the ESC OFF switch is engaged.