| VELOSTER(FS) >2013 > G 1.6 T-GDI > Body Electrical System > Rear Wiper/Washer > Rear Washer Motor>Repair procedures |

Inspection
1. | With the washer motor connected to the reservoir tank, fill the reservoir tank with water.
Before filling the reservoir tank with water, check the filter for foreign material or contamination. if necessary, clean the filter.
2. | Connect positive (+) and negative (-) battery cables to terminals 3 and 2 respectively.
3. | Check that the motor operates normally and the washer motor runs and water sprays from the rear nozzle.
4. | If they are abnormal, replace the washer motor.
Pin No. | Description
1 | Ground
2 | Front windshield washer (+)
3 | Rear windshield washer (+)