| VELOSTER(FS) >2013 > G 1.6 T-GDI > Engine Electrical System > Charging System > Alternator>Specifications |

Specification
Alternator
Item | Specification
Rated voltage | 13.5V, 110A
Speed in use | 1,000 ~ 18,000 rpm
Voltage regulator | IC Regulator built-in type
Regulator Setting Voltage | External mode | Refer to below graph
Internal mode | 14.55 ± 0.3V
Temperature Gradient | External mode | 0 ± 3 mV / °C
Internal mode | -3.5 ± 2mV / °C
※ Regulator Setting Voltage (External mode)