| VELOSTER(FS) >2013 > G 1.6 T-GDI > Clutch System > Clutch System > Concentric Slave Cylinder Assembly>Repair procedures |

Removal
1. | Remove the transaxle assembly. (Refer to Manual Transaxle System - " Manual Transaxle")
2. | Remove the concentric slave cylinder assembly from the transaxle case by removing bolts (A).
Tightening torque: 19.6 ~ 26.5 N.m (2.0 ~ 2.7 kgf.m, 14.5 ~ 19.5 lb-ft)
Installation
• | Install the concentric slave cylinder bolts. Not to be bent or twisted, Tighten them in diagonal directions.
• | When it is assembled, it must be free from invasive foreign matters and oil leakage.
1. | Installation is in reverse order of removal.
2. | Perform bleeding air procedure in concentric slave cylinder after pouring the brake fluid. (Refer to Concentric Slave Cylinder Assembly - "Adjustment")
Adjustment
Concentric Slave Cylinder Air Bleeding Procedure
1. | After disconnecting a cap from the concentric slave cylinder air bleeder, insert a vinyl hose in the plug.
2. | Refill the reservoir tank with the specified fluid.
Use the specified fluid. Avoid mixing different brands of fluid.
Specified fluid: SAE J1703 (DOT 3 or DOT 4)
3. | Pump the clutch pedal about 10 times.
4. | Loosen the air bleed screw (A) at hold down the clutch pedal to allow air to escape from the clutch system. Then tighten the air bleed screw.
5. | Repeat the step 2 ~ 4 until there is no bubble in the fluid.