| VELOSTER(FS) >2013 > G 1.6 T-GDI > Clutch System > General Information>Specifications |

Specifications
Items | Specifications
Clutch operation method | Hydraulic type
Clutch cover | Type | Diaphragm spring strap
Clutch disc Type | Type | Single dry with diaphragm
Faling diameter (Outer × inner) | Ø210 × Ø145 (Ø8.2677 × Ø5.7087)
Clutch release cylinder | inner diameter | 20.64 mm (0.8126 in.)
Clutch master cylinder | inner diameter | 15.87 mm (0.6248 in.)
Service Standard
Item | Specification
Clutch disc thickness [When free] | 8.3 ± 0.3 mm (0.3268 ± 0.0118 in.)
Clutch pedal height [With carpet] | 194.5 mm (7.6575 in.)
Clutch pedal free play | 7 ~ 10 mm (0.2756 ~ 0.3937 in.)
Clutch pedal stroke | 130 ± 0.3 mm (5.1181 ± 0.0118 in.)
Clutch disc rivet depth | 1.1 mm (0.0433 in.)
Diaphragm spring end height difference | 0.5 mm (0.0197 in.)
Clutch master cylinder clearance to piston | 1.6 mm (0.0630 in.)
Tightening Torques
Item | N.m | kgf.m | lb-ft
Clutch pedal mounting bolts & nuts | 18.6 ~ 23.5 | 1.9 ~ 2.4 | 13.7 ~ 17.4
Clutch release cylinder installation nut | 14.7 ~ 21.6 | 1.5 ~ 2.2 | 10.8 ~ 15.9
Clutch release cylinder union bolt | 24.5 ~ 34.3 | 2.5 ~ 3.5 | 18.1 ~ 25.3
Clutch release cylinder bleed plug | 6.8 ~ 9.8 | 0.7 ~ 1.0 | 9.2 ~ 13.3
Clutch cover mounting bolt | 14.7 ~ 21.6 | 1.5 ~ 2.2 | 10.8 ~ 15.9
Lubricants
Items | Specified lubricants | Quantity
Input shaft spline | CASMOLY L9508 | 0.2g
clutch release cylinder assembly | Brake fluid DOT 3 or DOT | As required
Clutch pedal shaft and bushings | Chassis grease SAE J310a, NLGI No.1