| VELOSTER(FS) >2013 > G 1.6 T-GDI > Engine Electrical System > Cruise Control System > Cruise Control Switch>Repair procedures |

Removal
1. | Disconnect the battery negative terminal.
2. | Remove the driver airbag module. (Refer to Restraint - "Airbag Module")
3. | Remove the steering wheel. (Refer to Steering System - "Steering Column and Shaft")
4. | Remove the steering wheel cover (A) after loosening the screws.
5. | Disconnect the audio switch connector (A).
6. | Disconnect the cruise control switch connector (A) and the trip switch connector (B).
7. | Disconnect the wiring (A) and then loosen the screws.
8. | Remove the steering wheel remote control switch assembly (A).
9. | Remove the cruise control switch (A).
Be careful not to damage the hook when removing the switch.
Installation
1. | Install in the reverse order of removal.
Inspection
[Measuring Resistance]
1. | Disconnect the cruise control switch connector from the control switch.
2. | Measure resistance between terminals on the control switch when each function switch is ON (switch is depressed).
Function switch | Terminal | Resistance
CANCEL | 3 - 4 | 180Ω ± 5%
SET/– | 3 - 4 | 330Ω ± 5%
RES/+ | 3 - 4 | 550Ω ± 5%
ON/OFF | 3 - 4 | 880Ω ± 5%
3. | If not within specification, replace switch.
[Measuring Voltage]
1. | Connect the cruise control switch connector to the control switch.
2. | Measure voltage between terminals on the harness side connector when each function switch is ON (switch is depressed).
Function switch | Terminal | Voltage
CANCEL | 3 - 4 | 0.66 ~ 0.86V
SET/– | 3 - 4 | 1.09 ~ 1.39V
RES/+ | 3 - 4 | 1.57 ~ 1.97V
ON/OFF | 3 - 4 | 2.12 ~ 2.56V
3. | If not within specification, replace switch.