| VELOSTER(FS) >2013 > G 1.6 T-GDI > Engine Mechanical System > Lubrication System > Oil Cooler>Repair procedures |

Removal
1. | Loosen the drain plug and drain the coolant. Open the radiator cap to make rapid draining. (Refer to Cooling System - "Coolant")
2. | Disconnect the oil cooler hose(A).
3. | Remove the oil filter(A) with the SST(09263-2E000, the oil filter wrench).
4. | Loosen the mounting bolt(A), and then remove the oil cooler(B).
Installation
1. | Apply a light coat of engine oil to the oil cooler packing surface (A), and then install the oil cooler(C) with fix bolt (B).
Tightening torque : 50.0 ~ 55.8 N.m (5.1 ~ 5.7kgf.m, 36.8 ~ 41.2 lb-ft)
2. | Install the oil filter(A) with the SST(09263-2E000, the oil filter wrench).
Tightening torque : 11.7 ~ 15.6 N.m (1.2 ~ 1.6kgf.m, 8.6 ~ 11.5 lb-ft)
3. | Install the oil cooler(A).
4. | Fill the radiator with coolant and check for leaks.