| VELOSTER(FS) >2013 > G 1.6 T-GDI > Fuel System > Engine Control System > ETC (Electronic Throttle Control) System>Troubleshooting |

Fail-Safe Mode
Item | Fail-Safe
ETC Motor | Throttle valve stuck at 7°
TPS | TPS 1 fault | ECM looks at TPS2
TPS 2 fault | ECM looks at TPS1
TPS 1,2 fault | Throttle valve stuck at 7°
APS | APS 1 fault | ECM looks at APS 2
APS 2 fault | ECM looks at APS 1
APS 1,2 fault | Engine idle state
When throttle value is stuck at 7°, engine speed is limited at below 1,500rpm and vehicle speed at maximum 40 ~ 50 km/h (25 ~ 31 mph)