| VELOSTER(FS) >2013 > G 1.6 T-GDI > Body Electrical System > Smart key System>Specifications |

Specification
Smart Key Unit
Items | Specification
Rated voltage | DC 12V
Operating voltage | DC 9 ~ 16V
Operating temperature | -30°C ~ 75°C (-22°F ~ 167°F)
Load | Max. 5mA (When welcome light frunction off)
Smart Key FOB
Items | Specification
Battery | Lithium battery 3V 1EA
Distance | 30m from vehicle, RF : 30m, Passive(LF) : 0.7m
Battery life | More than 2years (10 times / a day)
Push buttons | 4 (Door lock / unlock, Trunk lid, Panic)
Frequency(Rx) | 125 kHz
Frequency(Tx) | 315 MHz
Numbers | 2EA
Antenna
Items | Specification
Rated voltage | DC 12V
Operating voltage | DC 9 ~ 16V
Operating temperature | -30°C ~ 75°C (-22°F ~ 167°F)
Frequency | 125kHz
Numbers | Interior(3EA), Door(2EA), Bumper(1EA)